ARK PEST CONTROL 
Control of Substances Hazardous to Health (COSHH) Assessment – APC87

Product Name: (Purchased product brand name)




`
                 Reference No: 1

This COSHH Assessment form is solely for purchased hazardous substances 

Hazards identified on the container or Safety Data Sheet (SDS)
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Hazard/Risks Identification:

	None stated
No hazard pictogram, no signal word, no hazard statement(s), no precautionary statement(s) required


A brief description of how the substance is to be used:

	Hand application


Who is likely to be affected by the substance?

	Employees
	√
	Visitors
	√

	Cleaners
	√
	Patients / Residents / Service Users / Clients
	√

	General Public
	√
	Contractors
	√


Existing Controls (Provide a brief description of how the hazards are currently controlled. You may use the MSDS as a guide)

	Respiratory protection - If adequate local exhaust ventilation is not available or expo sure assessment demonstrates exposures outside the recommended guidelines, use respiratory protection. Equipment should conform to EN 143. Particulates type (P)
Hand protection – Material : Nitrile rubber Break through time : > 480 min

Eye protection - Safety glasses Equipment should conform to BS EN 166
Skin protection - Skin should be washed after contact.


Current storage arrangements and the quantity held in stock (Consider the risk of fire when storing substances. The fire risk must be covered in a separate Fire Risk Assessment)

	Keep in properly labelled containers. Store in accordance with the particular national regulations. 

Do not get on skin or clothing. Avoid breathing dust, fume, gas, mist, vapours or spray. Do not swallow. Avoid contact with eyes. Handle in accordance with good industrial hygiene and safety practice, based on the results of the workplace exposure assessment Take care to prevent spills, waste and minimize release to the environment.


Current Spillage/Release Arrangements.
	Avoid release to the environment. Prevent further leakage or spillage if safe to do so. Retain and dispose of contaminated wash water. If spillage enters rivers or watercourses, inform the Environment Agency (emergency telephone number 0800 807060).
Soak up with inert absorbent material. For large spills, provide dyking or other appropriate containment to keep material from spreading. If dyked material can be pumped, store recovered material in appropriate container. Clean up remaining materials from spill with suitable absorbent. Local or national regulations may apply to releases and disposal of this material, as well as those materials and items employed in the cleanup of releases. You will need to deter mine which regulations are applicable. 


Current Disposal Arrangements. (You may use the SDS as a guide but also consider residual left in the containers)

	Advice may be obtained from the local waste regulation authority (part of the Environment Agency in the UK).
Please follow container label instructions and applicable local guidelines.



Can the substance be removed or replaced by a substance less hazardous?
 YES / NO

How often do employees and others come into contact with the substance?

	Continual use
	
	Frequent use
	√
	Minimal use
	


Using this information, it is now possible to determine the level of risk from the substance and decide on the controls required to remove or reduce the risks.

Do you consider the current control measures suitable and sufficient? 

YES / NO 

EMERGENCY ARRANGEMENTS:

Fire Measures: What fire fighting measures are required to extinguish the substance? This information will be indicated on the safety data sheet if applicable.

	WATER FOG
	FOAM
	DRY POWDER
	CO2
	 CHEMICAL
	NONE

	√

	√
(alcohol resistant)
	√
	√
	
	


What methods are used to fire fight without putting yourself at risk? Is suitable PPE required and if so what?

	Use extinguishing measures that are appropriate to local circumstances and the surrounding environment. Use water spray to cool unopened containers. Remove undamaged containers from fire area if it is safe to do so. Evacuate area.



First Aid Measures: These are the first aid measures required should contact with the substance arise. It identifies each route of entry to the body and indicates what action must be taken should somebody become exposed. This information will be indicated on the safety data sheet.

Route of entry:




First Aid Measures:


	General advice:
	In the case of accident or if you feel unwell, seek medical ad vice immediately. When symptoms persist or in all cases of doubt seek medical advice.

	Inhalation:
	If inhaled, remove to fresh air. Get medical attention if symptoms occur.

	Absorption:
	n/a

	Ingestion:
	If swallowed, DO NOT induce vomiting. Get medical attention if symptoms occur. Rinse mouth thoroughly with water.

	Injection:
	n/a

	Skin Contact:
	Wash with water and soap as a precaution. Get medical attention if symptoms occur.

	Eye Contact:
	Flush eyes with water as a precaution. Get medical attention if irritation develops and persists.


Indication of any immediate medical attention and special treatment needed: None

Are the first aiders aware of the arrangements to deal with this substance in the event of a first aid emergency? 
YES / NO
Are there arrangements in place to deal with spillages? (eg is there an emergency procedure)?

 YES / NO
If you consider the controls adequate then sign the CoSHH assessment off. If further controls are required then identify them below. This CoSHH assessment must be reviewed at least annually. The CoSHH assessment must also be reviewed if there are any changes in circumstances and following an accident or incident.

Extra controls required to reduce the risks.


Identify the persons who are required to implement the extra controls and set a realistic date for completion of these extra controls.

	Action to be implemented by:
	Target Date:
	Completed Date:

	n/a
	
	

	
	
	


	Initial Assessment Completed By:
	Name:
	Signature:
	Date:

	
	Andy Owden
	A. Owden
	09.08.2026


ASSESSMENT REVIEW PROGRAM

	Assessment Review

Completed by:
	Name
	Signature
	Date

	
	
	
	

	Reason for review:
	Annual Review
	
	Changes
	
	Accident/Incident
	


	Assessment Review

Completed by:
	Name
	Signature
	Date

	
	
	
	

	Reason for review:
	Annual Review
	
	Changes
	
	Accident/Incident
	


	Assessment Review

Completed by:
	Name
	Signature
	Date

	
	
	
	

	Reason for review:
	Annual Review
	
	Changes
	
	Accident/Incident
	


MANUFACTURER/SUPPLIER OF MSDS SHEET:

Environmental Science FR SAS 

Milton Hall, 

Ely Rd., 

Milton 

Cambridge,

CB24 6WZ 

United Kingdom 

0800-1214-9451 (UK)
Rev: 04.08.2023





Harmonix Monitoring Paste	





If exposure to chemical is likely during typical use, provide eye flushing systems and safety showers close to the working place. When using do not eat, drink or smoke. Wash contaminated clothing before re-use.








APC88

